{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["Tex-436-A","RX"],"not_rendered":{"charts":0,"images":2,"macros":1,"external_links":0,"defined_names":54,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Tex-436-A","index":0,"n_rows":50,"n_cols":11,"rows_kept":50,"cut":false,"hidden":false,"merged":[[14,3,14,8],[41,1,41,8],[42,1,42,8],[0,0,0,1],[12,7,12,8],[11,3,11,4],[12,3,12,4],[13,3,13,4],[15,3,15,8],[13,7,13,8],[16,7,16,8],[33,1,36,8],[16,3,16,4],[28,2,28,6],[29,2,29,6],[31,2,31,6],[50,1,50,3],[46,6,46,8],[39,1,40,8],[44,2,44,4],[43,2,43,4],[46,1,46,3],[11,7,11,8],[7,7,7,8],[10,7,10,8],[7,3,7,4],[8,3,8,4],[8,7,8,8],[10,3,10,4],[9,7,9,8],[9,3,9,4]]}
["TxDOT Manuals >",null,null,"Tex-436-A"]
[null,"TEXAS DEPARTMENT OF TRANSPORTATION",null,null,null,null,null,null,null,null,11]
[null,null,null,null,null,null,null,null,null,null,1]
[null,null,null,null,null,null,null,null,null,null,"tx436.xlsm::45575.636412"]
[null,"MEASURING TEXTURE DEPTH BY THE SAND PATCH METHOD"]
[null,"Tex-436-A "]
[null,null,null,null,null,null,null,null,{"$f":"\"File Version: \" & TEXT(MID(sn,SEARCH(\"::\",sn,1)+2,20),\"mm/dd/yy hh:mm:ss\")","v":"File Version: 10/10/24 15:16:26"}]
[null,null,"SAMPLE ID:",null,null,null,"SAMPLED DATE:"]
[null,null,"TEST NUMBER:",null,null,null,"LETTING DATE:"]
[null,null,"SAMPLE STATUS:",null,null,null,"CONTROLLING CSJ:"]
[null,null,"COUNTY:",null,null,null,"SPEC YEAR:"]
[null,null,"SAMPLED BY:",null,null,null,"SPEC ITEM:"]
[null,null,"SAMPLE LOCATION:",null,null,null,"SPECIAL PROVISION:"]
[null,null,"MATERIAL CODE:",null,null,null,"GRADE:"]
[null,null,"MATERIAL NAME:"]
[null,null,"PRODUCER:"]
[null,null,"AREA ENGINEER:",null,null,null,"PROJECT MANAGER:"]
[]
[null,null,"COURSE\\LIFT:",null,"STATION:",null,null,"DIST. FROM CL:"]
[]
[]
[null,"Calculations"]
[]
[null,"Determine the texture depth T as follows:"]
[]
[]
[]
[null,"Where:"]
[null,null,{"$f":"\"V = the exact volume of the metal cylinder in (\"&IF(SpecYear=\"1995\",\"mL\",\"cubic inches)\")","v":"V = the exact volume of the metal cylinder in (cubic inches)"},null,null,null,null,null,"¨ "]
[null,null,{"$f":"\"D = the average diameter of the sand patch in (\"&IF(SpecYear=\"1995\",\"mm\",\"inches\") & \").\"","v":"D = the average diameter of the sand patch in (inches)."},null,null,null,null,null,"¨ "]
[]
[null,null,{"$f":"\"T = the texture depth in (\"&IF(SpecYear=\"1995\",\"mm\",\"inches\") & \").\"","v":"T = the texture depth in (inches)."},null,null,null,null,{"$f":"IF(ISERROR((4*H29)/(PI()*(H30^2))),\"\",(4*H29)/(PI()*(H30^2)))","v":""},"¨ "]
[]
[null,"NOTE: A volume V of 24.6 mL (1.50 in.3) can be obtained by a cylinder 19.05 mm (0.75 in.) in inside diameter and 86.36 mm (3.40 in.) in height. For quick reference, a conversion table relating sand patch diameters, D, to texture depths, T, can be determined for each sand patch test kit by using the above equation and the exact volume of the cylinder in the kit."]
[]
[]
[]
[]
[null,"Remarks:",{"$f":"NOW()","v":"2024-10-10T15:16:26.470"}]
[]
[]
[]
[]
[null,"Test Method:","Tested By:",null,null,"Tested Date:"]
[null,"TX436"]
[null,"Test Stamp Code:",null,null,"Omit Test:","Completed Date:","Reviewed By:"]
[]
[null,"Locked By:","TxDOT:","District:","Area:"]
[]
[null,"Authorized By:",null,null,"Authorized Date:"]

{"sheet":"RX","index":1,"n_rows":9,"n_cols":9,"rows_kept":9,"cut":false,"hidden":true,"merged":[]}
[7]
["Fld_nbr","Value","Desc_1","Desc_2","Desc_3","Desc_4","Desc_5","Desc_6","Desc_7"]
[1,{"$f":"IF('Tex-436-A'!$B$40=\"\",\"\",'Tex-436-A'!$B$40)","v":""},{"$f":"'Tex-436-A'!$B$39","v":"Remarks:"}]
[2,{"$f":"IF('Tex-436-A'!$D$19=\"\",\"\",'Tex-436-A'!$D$19)","v":""},{"$f":"IF('Tex-436-A'!$C$19=\"\",\"\",'Tex-436-A'!$C$19)","v":"COURSE\\LIFT:"}]
[3,{"$f":"IF('Tex-436-A'!$C$45=\"\",\"\",'Tex-436-A'!$C$45)","v":""},"Tested By ",{"$f":"IF('Tex-436-A'!$B$45=\"\",\"\",'Tex-436-A'!$B$45)","v":"TX436"}]
[4,{"$f":"IF('Tex-436-A'!$F$45=\"\",\"\",'Tex-436-A'!$F$45)","v":""},"Tested Date ",{"$f":"IF('Tex-436-A'!$B$45=\"\",\"\",'Tex-436-A'!$B$45)","v":"TX436"}]
[5,{"$f":"IF('Tex-436-A'!$H$29=\"\",\"\",'Tex-436-A'!$H$29)","v":""},{"$f":"IF('Tex-436-A'!$B$6=\"\",\"\",'Tex-436-A'!$B$6)","v":"Tex-436-A "},{"$f":"IF('Tex-436-A'!$C$29=\"\",\"\",'Tex-436-A'!$C$29)","v":"V = the exact volume of the metal cylinder in (cubic inches)"}]
[6,{"$f":"IF('Tex-436-A'!$H$30=\"\",\"\",'Tex-436-A'!$H$30)","v":""},{"$f":"IF('Tex-436-A'!$B$6=\"\",\"\",'Tex-436-A'!$B$6)","v":"Tex-436-A "},{"$f":"IF('Tex-436-A'!$C$30=\"\",\"\",'Tex-436-A'!$C$30)","v":"D = the average diameter of the sand patch in (inches)."}]
[7,{"$f":"IF('Tex-436-A'!$H$32=\"\",\"\",'Tex-436-A'!$H$32)","v":""},{"$f":"IF('Tex-436-A'!$B$6=\"\",\"\",'Tex-436-A'!$B$6)","v":"Tex-436-A "},{"$f":"IF('Tex-436-A'!$C$32=\"\",\"\",'Tex-436-A'!$C$32)","v":"T = the texture depth in (inches)."}]